{
	x: 6.0d,
	y: -1.0d,
	text: [
		"The compression dynamy accepts a variety of fluid inputs to produce RF. ",
		"Generally, the more steps it takes to obtain the fluid, the higher the energy output."
	],
	dependencies: [
		"fac6a69a"
	],
	tasks: [{
		uid: "146972cc",
		type: "item",
		items: [{
			id: "thermalexpansion:dynamo",
			tag: {
				RSControl: 0b,
				Facing: 1b,
				Energy: 0,
				Level: 0b
			},
			Damage: 2s
		}]
	}]
}
